,_distributed by##OTHER##,_current revision##OTHER##,_created by##OTHER##,_authorized by##OTHER##,_BIMspec_GUID##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabor##OTHER##,WarrantyDescription##OTHER##,Uniclass2##OTHER##,URL##OTHER##,TypeName##OTHER##,Type Comments##OTHER##,Type##OTHER##,Test Point Centre##LENGTH##MILLIMETERS,Test Point Base Radius##LENGTH##MILLIMETERS,Test Point Base Offset##LENGTH##MILLIMETERS,TagNumber##OTHER##,Suitable Pipe Applications##OTHER##,Square Disk##OTHER##,SpareParts##OTHER##,Size##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,Round Disk##OTHER##,Round Diameter##LENGTH##MILLIMETERS,ReplacementCost##OTHER##,ReferencedStandard##OTHER##,ProductionYear##OTHER##,Product Page Link##OTHER##,Product Documentation Link##OTHER##,Pressure Rating##OTHER##,Plug Radius##LENGTH##MILLIMETERS,Plug Length##LENGTH##MILLIMETERS,Plug Centres##LENGTH##MILLIMETERS,Pipe Size##LENGTH##MILLIMETERS,Pipe Radius##LENGTH##MILLIMETERS,Orifice Plate##OTHER##,Order Number##OTHER##,Nut Material##OTHER##,Nut Diameter##LENGTH##MILLIMETERS,Name with Orifice##OTHER##,Name No Orifice##OTHER##,ModelNumber##OTHER##,Model##OTHER##,Minimum Operating Temperature##OTHER##,Maximum Operating Temperature##OTHER##,Maximum Operating Pressure##OTHER##,Material##OTHER##,Manufacturer##OTHER##,L##LENGTH##MILLIMETERS,Keynote##OTHER##,K Coefficient##OTHER##,InstallationDate##OTHER##,Handle Radius##LENGTH##MILLIMETERS,Handle Depth##LENGTH##MILLIMETERS,Handle##OTHER##,H2##LENGTH##MILLIMETERS,H1##LENGTH##MILLIMETERS,Grade##OTHER##,Flange Thickness##LENGTH##MILLIMETERS,Finish##OTHER##,Features##OTHER##,Extidentifier##OTHER##,ExpectedLife##OTHER##,DurationUnit##OTHER##,DocumentationTechnical##OTHER##,DocumentationMaintenance##OTHER##,DocumentationLiterature##OTHER##,DocumentationInstallationGuide##OTHER##,DocumentationCertificates##OTHER##,Description##OTHER##,D##LENGTH##MILLIMETERS,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Color##OTHER##,CodePerformance##OTHER##,ClassificationValue##OTHER##,ClassificationName##OTHER##,Body Upper Offset##LENGTH##MILLIMETERS,Body Upper Depth##LENGTH##MILLIMETERS,Body Material##OTHER##,Body Lower Radius##LENGTH##MILLIMETERS,Body Centre Radius Offset##LENGTH##MILLIMETERS,Body Centre Curve Radius##LENGTH##MILLIMETERS,Body##OTHER##,BarCode##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Assembly Code##OTHER##,AccessibilityPerformance##OTHER##
DN65 (1 4218 71),www.bimstore.co.uk,1,Mark Thompson,Kris Atkinson,0,,,,Years,,,,Pr_65_54_95_26,http://www.herzvalves.com/www/default.asp,65mm Circuit Regulating Valve,65mm Circuit Regulating Valve,1,211.678832116788,15.000000000000,69.000000000000,,,1,,65 mm,,,0,150.000000000000,,,2015,http://www.herzvalves.com/www/default.asp?contentID=650,http://www.herzvalves.com/www/default.asp?contentID=650,PN16,14.000000000000,72.000000000000,178.000000000000,65.000000000000,32.500000000000,0,1 4218 71,Herz-Blue_Iron,19.000000000000,1 4218 71CS,1 4218 71,1 4218 71,Circuit Regulating Valve,-10 °C,130 °C,16 bar,Grey Cast Iron,Herz Valves UK Ltd,290.000000000000,S51,75,,75.000000000000,61.500000000000,Herz-Handle_Red,279.000000000000,186.000000000000,,20.000000000000,Painted Iron,,,0,Years,http://www.herzvalves.com/www/default.asp?contentID=650,,http://www.herzvalves.com/www/default.asp?contentID=650,,,"Circuit Regulating Valve for differential pressure measurement, with test points, flanged version",150.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_26,Uniclass2015,93.500000000000,31.000000000000,Herz-Blue_Iron,58.000000000000,210.000000000000,290.000000000000,Grey Cast Iron,,Fixed,,D30,
DN80 (1 4218 72),www.bimstore.co.uk,1,Mark Thompson,Kris Atkinson,0,,,,Years,,,,Pr_65_54_95_26,http://www.herzvalves.com/www/default.asp,80mm Circuit Regulating Valve,80mm Circuit Regulating Valve,2,226.277372262774,15.000000000000,85.000000000000,,,1,,80 mm,,,0,175.000000000000,,,2015,http://www.herzvalves.com/www/default.asp?contentID=650,http://www.herzvalves.com/www/default.asp?contentID=650,PN16,14.500000000000,81.000000000000,200.000000000000,80.000000000000,40.000000000000,0,1 4218 72,Herz-Blue_Iron,19.000000000000,1 4218 72CS,1 4218 72,1 4218 72,Circuit Regulating Valve,-10 °C,130 °C,16 bar,Grey Cast Iron,Herz Valves UK Ltd,310.000000000000,S51,110,,87.500000000000,63.333333333333,Herz-Handle_Red,307.000000000000,208.000000000000,,22.000000000000,Painted Iron,,,0,Years,http://www.herzvalves.com/www/default.asp?contentID=650,,http://www.herzvalves.com/www/default.asp?contentID=650,,,"Circuit Regulating Valve for differential pressure measurement, with test points, flanged version",175.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_26,Uniclass2015,110.000000000000,34.666666666667,Herz-Blue_Iron,62.000000000000,245.000000000000,335.000000000000,Grey Cast Iron,,Fixed,,D30,
DN100 (1 4218 73),www.bimstore.co.uk,1,Mark Thompson,Kris Atkinson,0,,,,Years,,,,Pr_65_54_95_26,http://www.herzvalves.com/www/default.asp,100mm Circuit Regulating Valve,100mm Circuit Regulating Valve,3,255.474452554745,15.000000000000,109.000000000000,,,1,,100 mm,,,0,175.000000000000,,,2015,http://www.herzvalves.com/www/default.asp?contentID=650,http://www.herzvalves.com/www/default.asp?contentID=650,PN16,11.700000000000,93.000000000000,236.000000000000,100.000000000000,50.000000000000,0,1 4218 73,Herz-Blue_Iron,19.000000000000,1 4218 73CS,1 4218 73,1 4218 73,Circuit Regulating Valve,-10 °C,130 °C,16 bar,Grey Cast Iron,Herz Valves UK Ltd,350.000000000000,S51,165,,87.500000000000,71.533333333333,Herz-Handle_Red,344.000000000000,235.000000000000,,24.000000000000,Painted Iron,,,0,Years,http://www.herzvalves.com/www/default.asp?contentID=650,,http://www.herzvalves.com/www/default.asp?contentID=650,,,"Circuit Regulating Valve for differential pressure measurement, with test points, flanged version",175.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_26,Uniclass2015,124.300000000000,39.166666666667,Herz-Blue_Iron,70.000000000000,310.000000000000,415.000000000000,Grey Cast Iron,,Fixed,,D30,
DN125 (1 4218 74),www.bimstore.co.uk,1,Mark Thompson,Kris Atkinson,0,,,,Years,,,,Pr_65_54_95_26,http://www.herzvalves.com/www/default.asp,125mm Circuit Regulating Valve,125mm Circuit Regulating Valve,4,291.970802919708,15.000000000000,128.000000000000,,,0,,125 mm,,,1,265.000000000000,,,2015,http://www.herzvalves.com/www/default.asp?contentID=650,http://www.herzvalves.com/www/default.asp?contentID=650,PN16,17.500000000000,110.000000000000,280.000000000000,125.000000000000,62.500000000000,0,1 4218 74,Herz-Blue_Iron,24.000000000000,1 4218 74CS,1 4218 74,1 4218 74,Circuit Regulating Valve,-10 °C,130 °C,16 bar,Grey Cast Iron,Herz Valves UK Ltd,400.000000000000,S51,241,,132.500000000000,72.566666666667,Herz-Handle_Red,385.000000000000,260.000000000000,,26.000000000000,Painted Iron,,,0,Years,http://www.herzvalves.com/www/default.asp?contentID=650,,http://www.herzvalves.com/www/default.asp?contentID=650,,,"Circuit Regulating Valve for differential pressure measurement, with test points, flanged version",265.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_26,Uniclass2015,144.100000000000,43.333333333333,Herz-Blue_Iron,80.000000000000,350.000000000000,470.000000000000,Grey Cast Iron,,Fixed,,D30,
DN150 (1 4218 75),www.bimstore.co.uk,1,Mark Thompson,Kris Atkinson,0,,,,Years,,,,Pr_65_54_95_26,http://www.herzvalves.com/www/default.asp,150mm Circuit Regulating Valve,150mm Circuit Regulating Valve,5,350.364963503650,30.000000000000,145.000000000000,,,0,,150 mm,,,1,265.000000000000,,,2015,http://www.herzvalves.com/www/default.asp?contentID=650,http://www.herzvalves.com/www/default.asp?contentID=650,PN16,20.000000000000,122.000000000000,340.000000000000,150.000000000000,75.000000000000,0,1 4218 75,Herz-Blue_Iron,24.000000000000,1 4218 75CS,1 4218 75,1 4218 75,Circuit Regulating Valve,-10 °C,130 °C,16 bar,Grey Cast Iron,Herz Valves UK Ltd,480.000000000000,S51,372,,132.500000000000,85.633333333333,Herz-Handle_Red,450.000000000000,310.000000000000,,26.000000000000,Painted Iron,,,0,Years,http://www.herzvalves.com/www/default.asp?contentID=650,,http://www.herzvalves.com/www/default.asp?contentID=650,,,"Circuit Regulating Valve for differential pressure measurement, with test points, flanged version",265.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_26,Uniclass2015,172.700000000000,51.666666666667,Herz-Blue_Iron,96.000000000000,465.000000000000,605.000000000000,Grey Cast Iron,,Fixed,,D30,
DN200 (1 4218 76),www.bimstore.co.uk,1,Mark Thompson,Kris Atkinson,0,,,,Years,,,,Pr_65_54_95_26,http://www.herzvalves.com/www/default.asp,200mm Circuit Regulating Valve,200mm Circuit Regulating Valve,6,444.444444444444,30.000000000000,190.000000000000,,,0,,200 mm,,,1,352.941176470588,,,2015,http://www.herzvalves.com/www/default.asp?contentID=650,http://www.herzvalves.com/www/default.asp?contentID=650,PN16,24.000000000000,150.000000000000,428.571428571429,200.000000000000,100.000000000000,0,1 4218 76,Herz-Blue_Iron,24.000000000000,1 4218 76CS,1 4218 76,1 4218 76,Circuit Regulating Valve,-10 °C,130 °C,16 bar,Grey Cast Iron,Herz Valves UK Ltd,600.000000000000,S51,704,,150.000000000000,113.333333333333,Herz-Handle_Red,569.000000000000,400.000000000000,,30.000000000000,Painted Iron,,,0,Years,http://www.herzvalves.com/www/default.asp?contentID=650,,http://www.herzvalves.com/www/default.asp?contentID=650,,,"Circuit Regulating Valve for differential pressure measurement, with test points, flanged version",450.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_26,Uniclass2015,220.000000000000,66.666666666667,Herz-Blue_Iron,120.000000000000,490.000000000000,660.000000000000,Grey Cast Iron,,Fixed,,D30,
DN250 (1 4218 77),www.bimstore.co.uk,1,Mark Thompson,Kris Atkinson,0,,,,Years,,,,Pr_65_54_95_26,http://www.herzvalves.com/www/default.asp,250mm Circuit Regulating Valve,250mm Circuit Regulating Valve,7,540.740740740741,30.000000000000,245.000000000000,,,0,,250 mm,,,1,429.411764705882,,,2015,http://www.herzvalves.com/www/default.asp?contentID=650,http://www.herzvalves.com/www/default.asp?contentID=650,PN16,28.000000000000,184.000000000000,521.428571428571,250.000000000000,125.000000000000,0,1 4218 77,Herz-Blue_Iron,24.000000000000,1 4218 77CS,1 4218 77,1 4218 77,Circuit Regulating Valve,-10 °C,130 °C,16 bar,Grey Cast Iron,Herz Valves UK Ltd,730.000000000000,S51,812,,160.000000000000,108.000000000000,Herz-Handle_Red,655.000000000000,453.000000000000,,32.000000000000,Painted Iron,,,0,Years,http://www.herzvalves.com/www/default.asp?contentID=650,,http://www.herzvalves.com/www/default.asp?contentID=650,,,"Circuit Regulating Valve for differential pressure measurement, with test points, flanged version",450.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_26,Uniclass2015,269.500000000000,75.500000000000,Herz-Blue_Iron,146.000000000000,820.000000000000,1025.000000000000,Grey Cast Iron,,Fixed,,D30,
DN300 (1 4218 78),www.bimstore.co.uk,1,Mark Thompson,Kris Atkinson,0,,,,Years,,,,Pr_65_54_95_26,http://www.herzvalves.com/www/default.asp,300mm Circuit Regulating Valve,300mm Circuit Regulating Valve,8,629.629629629630,30.000000000000,280.000000000000,,,0,,300 mm,,,1,500.000000000000,,,2015,http://www.herzvalves.com/www/default.asp?contentID=650,http://www.herzvalves.com/www/default.asp?contentID=650,PN16,32.000000000000,225.000000000000,607.142857142857,300.000000000000,150.000000000000,0,1 4218 78,Herz-Blue_Iron,24.000000000000,1 4218 78CS,1 4218 78,1 4218 78,Circuit Regulating Valve,-10 °C,130 °C,16 bar,Grey Cast Iron,Herz Valves UK Ltd,850.000000000000,S51,1383,,175.000000000000,114.333333333333,Herz-Handle_Red,783.000000000000,520.000000000000,,32.000000000000,Painted Iron,,,0,Years,http://www.herzvalves.com/www/default.asp?contentID=650,,http://www.herzvalves.com/www/default.asp?contentID=650,,,"Circuit Regulating Valve for differential pressure measurement, with test points, flanged version",450.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_26,Uniclass2015,319.000000000000,86.666666666667,Herz-Blue_Iron,170.000000000000,870.000000000000,1120.000000000000,Grey Cast Iron,,Fixed,,D30,
