,_distributed by##OTHER##,_current revision##OTHER##,_created by##OTHER##,_authorized by##OTHER##,_BIMspec_GUID##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabor##OTHER##,WarrantyDescription##OTHER##,URL##OTHER##,TypeName##OTHER##,Type Comments##OTHER##,Type##OTHER##,Two Inch##OTHER##,Three Quarter Inch##OTHER##,TagNumber##OTHER##,Swing Zone Mat##OTHER##,Swing Zone##OTHER##,Suitable Pipe Applications##OTHER##,Stop Height##LENGTH##MILLIMETERS,Stem Height##LENGTH##MILLIMETERS,SpareParts##OTHER##,Size##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,Sw##LENGTH##MILLIMETERS,ReplacementCost##OTHER##,ReferencedStandard##OTHER##,ProductionYear##OTHER##,Product O&M Link##OTHER##,Product Documentation Link##OTHER##,Pressure Rating##OTHER##,Pipe Size##LENGTH##MILLIMETERS,Pipe Radius##LENGTH##MILLIMETERS,Order Number##OTHER##,One Inch Body##OTHER##,One & One Quarter##OTHER##,One & One Half Body##OTHER##,ModelNumber##OTHER##,Model##OTHER##,Maximum Operating Temperature##OTHER##,Maximum Operating Pressure##OTHER##,Material##OTHER##,Manufacturer##OTHER##,L##LENGTH##MILLIMETERS,Keynote##OTHER##,K Coefficient##OTHER##,InstallationDate##OTHER##,Hex Thickness##LENGTH##MILLIMETERS,Hex Diameter##LENGTH##MILLIMETERS,Has Compression Fitting##OTHER##,Handle Position##LENGTH##MILLIMETERS,Handle Material##OTHER##,Half Inch Body##OTHER##,H##LENGTH##MILLIMETERS,Grade##OTHER##,Finish##OTHER##,Features##OTHER##,Extidentifier##OTHER##,ExpectedLife##OTHER##,DurationUnit##OTHER##,DocumentationTechnical##OTHER##,DocumentationMaintenance##OTHER##,DocumentationLiterature##OTHER##,DocumentationInstallationGuide##OTHER##,DocumentationCertificates##OTHER##,Description##OTHER##,A##LENGTH##MILLIMETERS,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Color##OTHER##,CodePerformance##OTHER##,ClassificationValue##OTHER##,ClassificationName##OTHER##,Body Material##OTHER##,BarCode##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Assembly Code##OTHER##,AccessibilityPerformance##OTHER##
DN15 (1 2190 01),www.bimstore.co.uk,1,Connor Laing,CL,0,,,,Years,,,,http://www.herzvalves.com/www/default.asp,Ball Valve,Ball Valve,3,0,0,,Clearance Zone,0,,67.800000000000,75.800000000000,,15mm,,,0.000000000000,,,2015,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,PN16,15.000000000000,7.500000000000,1 4017 01,0,0,0,1 4017 01,Herz Ball Valve With Extention Spindle ,130 °C at 10 bar,20 bar at 20 °C,Brass,Herz Valves UK Ltd,59.000000000000,S51,1.95,,12.000000000000,27.000000000000,0,22.355861934154,Herz Test Point - Red Plastic,1,90.000000000000,,,,,0,Years,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,,,Herz Ball Valve With Extention Spindle ,90.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_06,Uniclass 2015,Herz Brass,,Fixed,,D30,
DN20 (1 2190 02),www.bimstore.co.uk,1,Connor Laing,CL,0,,,,Years,,,,http://www.herzvalves.com/www/default.asp,Ball Valve,Ball Valve,4,0,1,,Clearance Zone,0,,70.800000000000,78.800000000000,,20mm,,,0.000000000000,,,2015,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,PN16,20.000000000000,10.000000000000,1 4017 02,0,0,0,1 4017 02,Herz Ball Valve With Extention Spindle ,130 °C at 10 bar,20 bar at 20 °C,Brass,Herz Valves UK Ltd,65.000000000000,S51,3.95,,12.500000000000,32.000000000000,0,25.000000000000,Herz Test Point - Red Plastic,0,93.000000000000,,,,,0,Years,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,,,Herz Ball Valve With Extention Spindle ,90.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_06,Uniclass 2015,Herz Brass,,Fixed,,D30,
DN25 (1 2190 04),www.bimstore.co.uk,1,Connor Laing,CL,0,,,,Years,,,,http://www.herzvalves.com/www/default.asp,Ball Valve,Ball Valve,5,0,0,,Clearance Zone,0,,84.800000000000,92.800000000000,,25mm,,,0.000000000000,,,2015,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,PN16,25.000000000000,12.500000000000,1 4017 03,1,0,0,1 4017 03,Herz Ball Valve With Extention Spindle ,130 °C at 10 bar,20 bar at 20 °C,Brass,Herz Valves UK Ltd,80.000000000000,S51,7.9,,17.000000000000,41.000000000000,0,32.000000000000,Herz Test Point - Red Plastic,0,107.000000000000,,,,,0,Years,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,,,Herz Ball Valve With Extention Spindle ,135.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_06,Uniclass 2015,Herz Brass,,Fixed,,D30,
DN32 (1 2190 04),www.bimstore.co.uk,1,Connor Laing,CL,0,,,,Years,,,,http://www.herzvalves.com/www/default.asp,Ball Valve,Ball Valve,6,0,0,,Clearance Zone,0,,88.800000000000,96.800000000000,,32mm,,,0.000000000000,,,2015,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,PN16,32.000000000000,16.000000000000,1 4017 04,0,1,0,1 4017 04,Herz Ball Valve With Extention Spindle ,130 °C at 10 bar,20 bar at 20 °C,Brass,Herz Valves UK Ltd,91.000000000000,S51,15.75,,18.000000000000,50.000000000000,0,38.000000000000,Herz Test Point - Red Plastic,0,111.000000000000,,,,,0,Years,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,,,Herz Ball Valve With Extention Spindle ,135.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_06,Uniclass 2015,Herz Brass,,Fixed,,D30,
DN40 (1 2190 05),www.bimstore.co.uk,1,Connor Laing,CL,0,,,,Years,,,,http://www.herzvalves.com/www/default.asp,Ball Valve,Ball Valve,7,0,0,,Clearance Zone,0,,113.800000000000,121.800000000000,,40mm,,,0.000000000000,,,2015,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,PN16,40.000000000000,20.000000000000,1 4017 05,0,0,1,1 4017 05,Herz Ball Valve With Extention Spindle ,130 °C at 10 bar,20 bar at 20 °C,Brass,Herz Valves UK Ltd,104.000000000000,S51,21.5,,18.000000000000,55.000000000000,0,45.000000000000,Herz Test Point - Red Plastic,0,136.000000000000,,,,,0,Years,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,,http://herzmediaserver.com/data/_www/srb/brosure/1401701_integral_fixed4_orifice_valve.pdf,,,Herz Ball Valve With Extention Spindle ,180.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_06,Uniclass 2015,Herz Brass,,Fixed,,D30,
DN50 (1 2190 06),www.bimstore.co.uk,1,Connor Laing,CL,0,,,,Years,,,,http://www.herzvalves.com/www/downloads/DS_2190_Ball_Valve.pdf,Ball Valve,Ball Valve,8,1,0,,Clearance Zone,0,,121.800000000000,129.800000000000,,50mm,,,0.000000000000,,,2015,http://www.herzvalves.com/www/downloads/DS_4017_M_FODRV.pdf,http://www.herzvalves.com/www/default.asp?contentID=644,PN16,50.000000000000,25.000000000000,1 4017 06,0,0,0,1 4017 06,Herz Ball Valve With Extention Spindle ,130 °C at 10 bar,20 bar at 20 °C,Brass,Herz Valves UK Ltd,125.000000000000,S51,46.7,,18.500000000000,70.000000000000,0,53.000000000000,Herz Test Point - Red Plastic,0,144.000000000000,,,,,0,Years,http://www.herzvalves.com/www/downloads/DS_2190_Ball_Valve.pdf,,http://www.herzvalves.com/www/downloads/DS_2190_Ball_Valve.pdf,,,Herz Ball Valve With Extention Spindle ,180.000000000000,April 2015,sales@herzvalves.com,,,,Pr_65_54_95_06,Uniclass 2015,Herz Brass,,Fixed,,D30,
